Optimization of Fluid Loading on Programmable Microfluidic Devices for Bio-protocol Execution